[Version]
Signature="$CHICAGO$"
Class=HDC
provider=%ZRAN%

[Manufacturer]
%MfgName%=Zoran

[Zoran]
%USB\VID_0595&PID_2002.DeviceDesc%=Coach.install,USB\VID_052B&PID_1819
%msd_\DISK.DeviceDesc%=msd_pdr.install,msd_\DISK

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
; \<WINDIR>\SYSTEM32\DRIVERS
msd_.files = 10,System32\Drivers

; \<WINDIR>\SYSTEM\IOSUBSYS
msd_pdr.files = 12

[Coach.install]
CopyFiles=msd_.files, msd_pdr.files
AddReg=msd_.addreg

[Coach.install.HW]
AddReg=bulkonly.addreg.HW

[msd_.addreg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,msd_.SYS


; Indicate that the device uses the C/B/I protocol
[cbi.addreg.HW]
HKR,,DeviceProtocol,0x10001,00

; Indicate that the device uses the C/B protocol
[cb.addreg.HW]
HKR,,DeviceProtocol,0x10001,01

; Indicate that the device uses the BULK ONLY protocol
[bulkonly.addreg.HW]
HKR,,DeviceProtocol,0x10001,50

; Install the port driver
[msd_pdr.install]
AddReg=msd_pdr.addreg

[msd_pdr.addreg]
HKR,,DevLoader,,*ios
HKR,,PortDriver,,msd_pdr.pdr

[msd_.files]
msd_.sys

[msd_pdr.files]
msd_pdr.pdr

[SourceDisksNames]
1000 = "USB Mass Storage Sample Driver Disk","",,

[SourceDisksFiles]
msd_.SYS = 1000
msd_PDR.PDR = 1000

;---------------------------------------------------------------;

[Strings]
ZRAN="DSC Manufacturer"
MfgName="DSC Manufacturer"
USB\VID_0595&PID_2002.DeviceDesc="USB MSDC"
msd_\DISK.DeviceDesc="Mass Storage Device"
